Rath, P., Vetter, A., Kovalyuk, V., Ferrari, S., Kahl, O., Nebel, C., et al. (2016). Travelling-wave single-photon detectors integrated with diamond photonic circuits: operation at visible and telecom wavelengths with a timing jitter down to 23 ps. In J. - E. Broquin, & G. N. Conti (Eds.), Integrated Optics: Devices, Mat. Technol. XX (Vol. 9750, pp. 135–142). Spie.